I-25078

**OC Subsection:** [[F-3688]](#3688) New OC Subsection: 06 Driving / Braking Systems

**Description:**

↵

Title: Disengaging Auto Vehicle Hold

Goal: Disengagingof auto vheicle hold

Scope:

* Brake and Aceleration pedals
* EPB
* Gear selector
* Doors
* Seat buckles

Actor: Driver

Preconditions:

AVH has been [engaged](#24695)

Triggers:

* The driver presses the accelerator pedal in\_22
* Press brake pedal in\_23
* Gear is shifted to R via in\_9 or in\_2
* Gear is shifted to P via in\_9 or in\_2
* Gear is shifted to N via in\_9 or in\_2
* Vehicle stay engaged in AVH for 10 minutes
* Driver's exit Vehicle - unbuckle the seat belt and open the door

Requirements:

* If the driver's exit vehicle - unbuckles the seat belt and opens the door, the EV is automatically shuffled to Park after AVH disengaged [LOOKS LIKE SEPARATE UC #6225]
* AVH setting is part of User Profile AVH is available only if One Pedal mode is disabled
* display AVH state (disengaged) on out\_2

**Priority:** Normal

**Type**: Use Case CF

#### Document

**Caption:** operational\_concept.Profile - 383201 Profiles settings

**Overall estimation:**

**Requirement type:** Profile

**Type**: Profile